{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":24,"n_cols":3,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[]
[]
["Tabelle für die Stabilitätsindex"]
[]
["Mastlänge",0,"m"]
["Mastgewicht pro m inkl stehendes und laufendes Gut *",0,"kg"]
["Rumphöhe",0,"m"]
["Kiellänge",0,"m"]
["Rumpfbreite inkl Ausleger/Foils",0,"m"]
["Rumpflänge",0,"m"]
["Kielbombe",0,"kg "]
[]
["W4",{"$f":"0.15*B10*B9","v":0}]
["W3",{"$f":"B6/2","v":0}]
["W1",{"$f":"(B14*(B5*B5)+B13)/(B8+0.5*B7)","v":{"$error":"#DIV/0!"}}]
["Drt",{"$f":"0.5*(B6)*(B4+B13)","v":0}]
["Moment*F",{"$f":"B15*1.5","v":{"$error":"#DIV/0!"}}]
["Stabilitätsindex",{"$f":"B15*3","v":{"$error":"#DIV/0!"}},"kg"]
["Bei einem roten Ergebnis muss ein Auftrieb am Masttop oder Segel installiert werden, um das Durchkentern zu verhindern."]
[]
[null,"Alu","Carbon"]
["*Beispiele Racer bis 10m","kg/m","kg/m"]
["Wert Racer mit Rodwanten",5.8,3.6]
["Wert Racer mit Textilwanten",null,2.9]